Vigilent GraphQL Queries and Mutations - Keywords used in the automation script

|  |  |  |
| --- | --- | --- |
| **#** | **gqlQuery /gqlMutation** | **gqlQuery/gqlMutation** |
| 1 | [configWriteMutation](#_configWriteMutation_-_Mutation) | gqlMutation |
| 2 | [pointWriteMutation](#_pointWriteMutation) | gqlMutation |
| 3 | [setSetPointLimits](#_setSetPointLimits_-_Mutation) | gqlMutation |
| 4 | [setGroupPropertymutation](#_setGroupPropertymutation_-_Mutation) | gqlMutation |
| 5 | [testEventLogMutation](#_testEventLogMutation) | gqlMutation |
| 6 | [setSFCMutation](#_setSFCMutation) | gqlMutation |
| 7 | [setBOPMutation](#_setBOPMutation) | gqlMutation |
| 8 | [releaseOverrideOfAllAHUsMutation](#_releaseOverrideOfAllAHUsMutation) | gqlMutation |
| 9 | [groupNameOidMutation](#_groupNameOidMutation) | gqlQuery |
| 10 | [getAHUStatusInGroupQuery](#_getAHUStatusInGroupQuery) | gqlQuery |
| 11 | [getCtrlStateValueQuery](#_getCtrlStateValueQuery) | gqlQuery |
| 12 | [getRackSensorPointsOfGroupQuery](#_getRackSensorPointsOfGroupQuery) | gqlQuery |
| 13 | [getAlarmStatusQuery](#_getAlarmStatusQuery) | gqlQuery |
| 14 | [getOverrideDetailsOfAHUsInGroup](#_getOverrideDetailsOfAHUsInGroup) | gqlQuery |
| 15 | [getSpecificSensorPointsOfGroupQuery](#_getSpecificSensorPointsOfGroupQuery) | gqlQuery |
| 16 | [getAHUsPropertiesOfSpecificGroup](#_getAHUsPropertiesOfSpecificGroup) | gqlQuery |
| 17 | [setGroupPropertymutation](#_setGroupPropertymutation) | gqlMutation |
| 18 | [getAHUsInMismatchState](#_getAHUsInMismatchState) | gqlQuery |
| 19 | [getAHUStateofAhuInGroup](#_getAHUStateofAhuInGroup) | gqlQuery |
|  |  |  |

GraphQL Queries / Mutations:

### configWriteMutation

This mutation is used to set the system properties in Tools->Configs->DASHM

e.g. Tools->Configs->DASHM-> Property Name – NumGuardUnits & value - 5

mutation configWrite {

configSet(requests: [{module: "DASHM", name: "NumGuardUnits", value: "5"}]) {

index

reason

}

}

### pointWriteMutation

This mutation is used to set the temperature of Rack Bottom or Rack Top with oid.

mutation pointWrite {

pointWrite(requests: [{oid: 2220, value: 66.78}]) {

index

reason

}

}

### setSetPointLimits

This mutation is used to set high limit temperature and low limit temperature for the Rack Top with oid.

mutation targetSetPoints {

targetSet(requests: [{oid: 2228, value: 80.8, target: LIMIT\_HIGH, origin: "MANUAL"}, {oid: 2228, value: 60.8, target: LIMIT\_LOW, origin: "MANUAL"}]) {

index

reason

}

}

### setGroupPropertymutation

This mutation is used to set group property value based on property name with group oid.

mutation setGrpProp {

propertyWrite(requests: [{oid: 598, name: "AllowNumExceedencesGuard", int: 8}]) {

index

reason

}

}

### testEventLogMutation

This mutation is used to set custom message for event log.

mutation TestEventLog {

eventLog(requests: [{source: "Ideavat AuQA", message: "message"}]) {

index

reason

}

}

### setSFCMutation

This mutation is used to set SFC value for an AHU with SFC oid.

mutation targetSetSFC {

targetSet(requests: [{oid: 676, value: 88, unit: percent100, target: CONTROL, origin: "MANUAL", priority: 70}]) {

index

reason

}

}

### setBOPMutation

This mutation is used to set BOP value for an AHU with BOP oid.

mutation targetSetBOP {

targetSet(requests: [{oid: 8440, value: 1, target: CONTROL, origin: "MANUAL", priority: 70}]) {

index

reason

}

}

### releaseOverrideOfAllAHUsMutation

This mutation is used to release all AHUs.

mutation targetClearOverride {

targetClear(requests: [{oid: 8440, target: CONTROL, origin: "MANUAL"}, {oid: 8456, target: CONTROL, origin: "MANUAL"}, {oid: 8472, target: CONTROL, origin: "MANUAL"}, {oid: 8488, target: CONTROL, origin: "MANUAL"}, {oid: 8504, target: CONTROL, origin: "MANUAL"}, {oid: 8520, target: CONTROL, origin: "MANUAL"}, {oid: 8536, target: CONTROL, origin: "MANUAL"}, {oid: 8552, target: CONTROL, origin: "MANUAL"}, {oid: 676, target: CONTROL, origin: "MANUAL"}, {oid: 767, target: CONTROL, origin: "MANUAL"}, {oid: 858, target: CONTROL, origin: "MANUAL"}, {oid: 949, target: CONTROL, origin: "MANUAL"}, {oid: 1040, target: CONTROL, origin: "MANUAL"}, {oid: 1131, target: CONTROL, origin: "MANUAL"}, {oid: 1222, target: CONTROL, origin: "MANUAL"}, {oid: 1313, target: CONTROL, origin: "MANUAL"}]) {

index

reason

}

}

### groupNameOidMutation

This query is used to fetch the group oid based on group name.

query getGroupOid {

site {

groups: children (selector: {type: Group, name: "General-test"}) {

oid

}

}

}

### getAHUStatusInGroupQuery

This query is used to fetch the all AHUs and their BOP & SFC oid’s based on group name.

query getAHUStatusInGroup {

site {

groups: children(selector: {type: Group, name: "General-test"}) {

oid

type

displayName

ahus: children(selector: {type: AHU}) {

oid

type

displayName

name

controls: search (selector: {target: CONTROL}, pruneDepth: false) {

oid

type

displayName

name

status: targetStatus(target: CONTROL) {

origin

}

}

}

}

}

}

### getCtrlStateValueQuery

This query is used to fetch the group’s control state value based on group name.

query getCtrlStateValue {

site {

groups: children(selector: {type: Group, name: "General-test"}) {

children(selector: {type: GroupStatus, name: "Group Status"}) {

children(selector: {type: State, name: "CtrlState"}) {

name

pointCurrent {

value

}

}

}

}

}

}

### getRackSensorPointsOfGroupQuery

This query is used to fetch the rack sensor points of a group based on group name.

query rackSensorPoints {

site {

groups: children(selector: {type: Group, name: "General-test"}) @skip(if: false) {

oid

name

racks: children(selector: {type: Rack}) {

oid

displayName

points: children {

oid

name

type

pointCurrent {

value

}

}

}

}

}

}

### getAlarmStatusQuery

This query is used to fetch the alarm’s status based on group name and alarm type.

query alarmStatus {

alarms(selector: {subjectName: "Imputes-test", type: GroupDeadSensor}) {

type

severity

status

}

}

### getOverrideDetailsOfAHUsInGroup

This query is used to fetch the AHU is in override state based on group name.

query overrideGet {

site {

groups: children(selector: {type: Group, name: " General-test"}) {

oid

name

ahus: children(selector: {type: AHU}) {

oid

name

controls: search(selector: {target: CONTROL}) {

oid

type

name

point: pointCurrent(unit: percent100) {

value

}

targetStatus(target: CONTROL, unit: percent100) {

requests {

status

origin

priority

value

unit

}

}

}

}

}

}

}

### getSpecificSensorPointsOfGroupQuery

This query is used to fetch the specific sensor points based on group name.

query getSpecificSensorPointDetails {

site {

name

groups: children(selector: {type: Group, name: "General-test"}) {

name

sensors: search(selector: {types: [RAT]}, maxResults: 9999) {

name

type

oid

pathName(details: true)

pointCurrent(units: [degF, kWe]) {

unit

value

tstamp

}

}

}

}

}

### getAHUsPropertiesOfSpecificGroup

This query is used to fetch the groups AHU’s properties based on group name and used in MinOn test.

query getGroupsAHUProperties {

site {

groups: children(selector: {type: Group, name: "General-test"}) {

name

ahus: children(selector: {type: AHU}) {

name

CoolSource: propString(name: "CoolSource")

DesignCapacity: prop(name: "DesignCapacity") {

value: float

unit

}

DesignCop: propFloat(name: "DesignCop")

}

}

}

} ​​

### setGroupPropertymutation

This mutation is used to set the group properties based on oid, property name and value to be set.

mutation setGrpProp {

propertyWrite(requests: [{oid: 35876, name: "FanCtrlMax", float: 0.5}]) {

index

reason

}

}

### getAHUsInMismatchState

This query is used to fetch the Ahu in mismatch state in the group.

query AHUMismatchInGroup {

site {

groups: children(selector: {type: Group, name: "${group\_name}"}) {

nameahus: children(selector: {type: AHU}) {

name

pointCurrent: children(selector: {name: "SyncFaultStatus"}) {

type

name

pathName

SyncFaultStatus: pointCurrent {

value

}

}

}

}

}

}

**Example** –

query AHUMismatchInGroup {

site {

groups: children(selector: {type: Group, name: "NoBindings"}) {

nameahus: children(selector: {type: AHU}) {

name

pointCurrent: children(selector: {name: "SyncFaultStatus"}) {

type

name

pathName

SyncFaultStatus: pointCurrent {

value

}

}

}

}

}

}

### getAHUStateofAhuInGroup

This query is used to fetch the AHU’s state in the group.

query getAHUStateofAhuInGroup { site { groups: children(selector: {type: Group, oid: ${group\_oid}}) { ahus: children(selector: {type: AHU}) { AHUState: prop(name: "AhuState") { name string }}}}}

**Example** -

query getAHUStateofAhuInGroup { site { groups: children(selector: {type: Group, oid: ${group\_oid}}) { ahus: children(selector: {type: AHU}) { AHUState: prop(name: "AhuState") { name string }}}}}